_______________________________
1- Introduction
 
The PL7-07 V4.0 programming CD-ROM is used to expand applications aimed at TSX Nano PLCs.

This CD-ROM contains the following elements:
 
 - PL7-07 V4.0 software for TSX Nano programming
 - New UNI-TELWAY drivers adapted to the different Windows versions and the new TSX PCU 1031 cable.
 - Technical documentation in 4 languages: French, English, German, Spanish.

_______________________________
1- New developments in PL7-07 version V4.0 software

 - The maximum number of TSX Nano MODBUS slaves is now 247.
 - Installing UNI-TELWAY drivers according to the operating environment has been extended and made easier.
 - Using the TSX PCU 1031 cable with its associated drivers means the range of usable PCs can be extended, 
   as well as the range of compatible environments (power management etc).

WARNING:
 
Following developments in the UNI-TELWAY DOS driver, operating PL7-07 V4.0 from Windows 3.1 is no longer possible.
You must exit Windows 3.1, then start PL7-07 in DOS.
It is recommanded of uninstall existing driver UNI-TELWAY to avoid 
any conflict of version under Win98, Win2000.

_____________________________
2- Installing PL7-07 version V4.0

Launch the file Install.exe. 
Confirm the information.

_______________________________
3- Installing the UNI-TELWAY driver in Win98, Win2000 and WinNT

To use the new UNI-TELWAY driver configuration tool, you must have already installed 
Microsoft Data Access Component V2.1. 
The software is included in this CDROM - launch the file mdac_typ.exe in the DRIVERS\MDAC directory.
 
_______________________________
4- Generating a disk set from PL7-07 software
  
If you want to generate a disk set to install PL7-07 on a PC without a CD-ROM drive, 
you must start the file Makedisk.bat in the CD ROM and follow the instructions displayed on the screen.

_______________________________
5- Installing PL7-07 software from the disk set.

Place disk DISK#1 in the disk drive.
Start the file Install.exe.
Confirm the information.

_______________________________
6- Generating a disk set from the UNI-TELWAY driver

Start the file Makedisk.bat from the DRIVERS\WIN9598 directory for the UNI-TELWAY Win95-Win98 driver.
Follow the instructions.

Start the file Makedisk.bat from the DRIVERS\WINNT directory for the UNI-TELWAY WinNT driver.
Follow the instructions.

Start the file Makedisk.bat from the DRIVERS\WIN2000 directory for the UNI-TELWAY Win2000 driver.
Follow the instructions.
 
_______________________________
7- Accessing the technical documentation

The pdf file in the "\Doc\English" CD-ROM directory contains the PL7-07 technical documentation.
This technical documentation is also available in other languages in their associated directories.
